Gold & Silver Forum (http://goldismoney.info/forums/index.php)
- Survival Prep (http://goldismoney.info/forums/forumdisplay.php?f=141)
- - purifying water. (http://goldismoney.info/forums/showthread.php?t=287704)

killer2021 | 07-31-2008 02:34 AM
purifying water. What is the most efficient, cheapest way to purify water? I want to take water from a source in nature like a lake, pond, or river and convert it to drinking water. There may be pollution in the river (animal waste, agriculture chemicals, oils, other chemicals etc.) So I need to be able to remove those. I want it to be a simple system, nothing complex or expensive. I want the system to produce, maybe 1 gallon of water per day.

killer2021 | 07-31-2008 04:58 AM
Re: purifying water. Another person also told me to use solar water distillation, basically heat the water turn into steam then condense the steam. How effective is that?

Saul Mine | 07-31-2008 09:29 AM
Re: purifying water. Quote:
Originally Posted by killer2021 (Post 1216709) Another person also told me to use solar water distillation, basically heat the water turn into steam then condense the steam. How effective is that?
Distillation is effective, but it takes a very large amount of heat to vaporize water. Obviously you need an equal amount of cooling, which not everybody considers. In a desert you have lots of heat but little cooling. The reverse is true in snow. There is almost always a better choice than distillation, except that it is the easiest to set up in primitive conditions. For instance, you can use a copper pipe pushed onto a pressure cooker, with an improvised cooling jacket on the pipe.

Ara | 07-31-2008 11:10 AM
Re: purifying water. http://www.boatus.com/goodoldboat/pressure.asp http://i13.photobucket.com/albums/a2...urelineart.jpg Making a distiller After some experimentation, our pressure cooker has become a successful distiller with the addition of these items: 10-feet of 1/4-inch outside diameter copper tubing two 3-foot lengths of 3/8-inch outside diameter (1/4-inch inside diameter) food-grade vinyl tubing two hose clamps a bucket a water container How we put the distiller together and run it: First, we fill the bucket with cool seawater and bring it below to our galley. Then we fill our pressure cooker 2/3 full with seawater or any other water that may or may not be contaminated. Our copper tubing is wound into a coil around something cylindrical so it will fit completely into the bucket of cool seawater with one end pointed up toward the pressure cooker on the stove. Our pressure cooker has a vent pipe with an outside diameter of 1/4-inch. We slide one of the 3-foot lengths of food-grade vinyl all the way onto the vent pipe in the lid. Then with a hose clamp over the vinyl tubing, we slide the copper tubing into the remaining loose end and tighten the clamp. The remaining piece of food-grade vinyl tubing attaches to the copper tubing end at the bottom of the bucket with a hose clamp as well. Then the remaining end of vinyl tubing is placed inside the water container, which sits next to the bucket. It helps if your container is shorter than your bucket. Now we are ready to assemble the pressure cooker and heat the seawater. As steam builds up inside the cooker, it begins to make its way through the tubing. When it reaches the copper coils, it condenses into pure water and flows into the water container. The key to making this distiller run efficiently is to replace the seawater in the bucket once it warms up. Be careful not to burn yourself when you lift the coil out of the bucket to change the water. As the flow develops, we turn the burner to medium low because less heat is required. Once the steam begins going through the tubing, we usually get about 1 cup of water after about 25 minutes on medium heat. Keeping the copper tubing in a coil with the vinyl tubing already attached helps with storing and quick assembly. Before using the tubing for the first time, rinse it with clean water. Be sure to use only food-grade tubing, as not all vinyl tubing is safe for drinking water use. We have never found the vinyl tubing to pop off the vent pipe or melt with the heat. The pressure that builds up is not the same because of the lack of the weighted regulator on the vent pipe, so the temperature is not as high either. If the power is off and you have a place to build a fire you can purify water, even seawater.

Ash_Williams | 07-31-2008 02:02 PM
Re: purifying water. Quote:
Another person also told me to use solar water distillation, basically heat the water turn into steam then condense the steam. How effective is that?
If you are trying to remove chemicals then this may not be the way to go. Some chemicals may have a lower boiling point than the water and end up in your final product.

buff01 | 07-31-2008 02:16 PM
Re: purifying water. http://en.wikipedia.org/wiki/Solar_still A solar oven could easily be converted into a solar still if you wanted to do so. Recycling urine can be fun and easy!

SLV>GLD | 07-31-2008 03:10 PM
Re: purifying water. Yes, I love to "arrange" my urine in sand.

All times are GMT -4. The time now is 10:07 AM. |

Powered by vBulletin® Version 3.8.4
Copyright ©2000 - 2010, Jelsoft Enterprises Ltd.
Copyright = None use it and Link to GIM