Gold & Silver Forum (http://goldismoney.info/forums/index.php)
- Firearms (http://goldismoney.info/forums/forumdisplay.php?f=159)
- - 5.45 Hollowpoint tests (http://goldismoney.info/forums/showthread.php?t=407272)

SilverCity | 09-13-2009 11:30 PM
5.45 Hollowpoint tests 4 Attachment(s) Some more results from modified Wolf ammo tests: 1) The modified Wolf fmj (into hollow points) fed perfectly from the ten-round factory mag. They DID NOT feed reliably with Bulgarian military 30-rounders...even with the bullet guide installed. 2) The hollowpoint accuracy to 100 yards is on par with the standard Wolf fmj out of the Saiga. 3) In repeated tests, the hollowpoint bullets fired from ~20 yards penetrated three 1/2gal water-filled milk cartons taped together (that's 12 inches minimum), destroying the first 2 cartons in the process. 4) The only bullets recovered were tiny fragments of steel jacket and lead core from inside the 3rd carton or scattered around on the ground. photos: a. exited side of 3rd carton b. example of recovered bullet fragments c. 3rd carton exit hole d. jug laid on end, shot through bottom, exit out the top

Lucky225 | 09-14-2009 06:00 PM
Re: 5.45 Hollowpoint tests thanks for sharing!

Lamentations | 09-14-2009 10:03 PM
Re: 5.45 Hollowpoint tests Seems like a lot of work if you intended to modify each round by hand, even for enough rounds to fill a magazine. Cant you get 5.45 HP ammo?

eat_beef | 09-14-2009 10:04 PM
Re: 5.45 Hollowpoint tests Cool. Looks like lack of penetration might not be a problem. Of course water in a milk jug isn't ordinance gelatin, but 12inches and still going aint bad. Do unmodified bullets run in the bulgy mags? Did you pop any jugs w/ 7n6 to compare?

SilverCity | 09-14-2009 10:20 PM
Re: 5.45 Hollowpoint tests Quote:
Originally Posted by Lamentations (Post 1921106) Seems like a lot of work if you intended to modify each round by hand, even for enough rounds to fill a magazine. Cant you get 5.45 HP ammo?
Once I got the process down, it only took about a minute or so to process each round. Used a flash hole reamer for the final tip clean-up. Factory hollow points are different in that they don't have the deep hollow cavity that my modified bullets do...but I haven't done any testing on them.

SilverCity | 09-14-2009 10:30 PM
Re: 5.45 Hollowpoint tests Quote:
Originally Posted by eat_beef (Post 1921107) Cool. Looks like lack of penetration might not be a problem. Of course water in a milk jug isn't ordinance gelatin, but 12inches and still going aint bad. Do unmodified bullets run in the bulgy mags? Did you pop any jugs w/ 7n6 to compare?
Unmodified bullets run perfectly throught Bulgarian mags. My HPs would probably work if I built up notch in the front edge of the '74 mags... Haven't popped any cartons with 7N6 yet...I'll let ya know when I do. SC

All times are GMT -4. The time now is 10:42 AM. |

Powered by vBulletin® Version 3.8.4
Copyright ©2000 - 2010, Jelsoft Enterprises Ltd.
Copyright = None use it and Link to GIM