Gold & Silver Forum (http://goldismoney.info/forums/index.php)
- Survival Prep (http://goldismoney.info/forums/forumdisplay.php?f=141)
- - In wall load center to on wall box (http://goldismoney.info/forums/showthread.php?t=376917)

TechGuy | 05-21-2009 03:39 PM
In wall load center to on wall box anyone have any pics or tips on how to transition from an in wall breaker box/load center to a wall mounted subpanel or conduit? I would like to be able to do this as cleanly as possible.

Professur | 05-21-2009 03:53 PM
Re: In wall load center to on wall box The Black and Decker Advanced Wiring handbook has very clear descriptions and photos of doing this, but I haven't had a scanner in years. Amazon Amazon

striped_bear | 05-21-2009 06:24 PM
Re: In wall load center to on wall box Quote:
Originally Posted by Professur (Post 1732524) The Black and Decker Advanced Wiring handbook has very clear descriptions and photos of doing this, but I haven't had a scanner in years. http://www.amazon.com/Black-Decker-A.../dp/0865737193
I just ordered that book a few days ago as I'm currently studying electricity and wiring. All the reviews I've read say it's indispensable.

TTAZZMAN | 05-22-2009 01:49 AM
Re: In wall load center to on wall box If it were me i would just come out of the bottom/side of the main.....into the back of the sub panel.....leaveing nothing exposed I would probably just slot the sheetrock below the main...and mount the sub over the slot to cover it...If i wanted to go to the side i would do the same thing but i would then have to repair the sheetrock (to me a sht rock repair is pretty minor) if i was going to a conduit.....i would do the same thing as above ..substituing a Jct box or a disconnect box for the sub panel then take a conduit off of the Jct box to whereever. it could be done with either romex or flex conduit ...i tend to prefer pulling through conduit myself i am assuming your asking a physical installation question and not a wiring diagram question? If its a wiring question....its really simple....breaker...correctly load sized wire......termination

TechGuy | 05-22-2009 10:18 AM
Re: In wall load center to on wall box 1 Attachment(s) This is what I am looking to do, just trying to get a better idea how to mount. Right now it is looking like a fire treated 3/4 inch plywood mounting board adjacent to my current in wall breaker box. I have lots of xp with electricity and wiring, just not as much with conduit, especially when doing transitions like this.

All times are GMT -4. The time now is 09:51 AM. |

Powered by vBulletin® Version 3.8.4
Copyright ©2000 - 2010, Jelsoft Enterprises Ltd.
Copyright = None use it and Link to GIM