Gold & Silver Forum (http://goldismoney.info/forums/index.php)
- Survival Prep (http://goldismoney.info/forums/forumdisplay.php?f=141)
- - ak47 question (http://goldismoney.info/forums/showthread.php?t=109422)

NOOB | 02-11-2007 08:56 PM
ak47 question I told you guys about the new ak underfolder I purchased. Well I like it so much I went back and bought a regular stock ak47. here is my question. On the yugo underfolder if you pull the bolt back it will staty back unless you pull it again and release. This is common on autoloaders to my knowledge. The romanian bolt will not stay back. Anybody know whats up with this? NOOB

Quixote2 | 02-11-2007 09:07 PM
Re: ak47 question Clean out more cosmoline in the action.

Tn...Andy | 02-11-2007 09:09 PM
Re: ak47 question I think it has to do with the magazine you have in it.....seems I've seen them for bolt open or not ....... Read here: http://www.ar15.com/lite/topic.html?b=4&f=55&t=84152

NOOB | 02-11-2007 09:19 PM
Re: ak47 question Thanks for the link TN, but I am talking about with the mag out. What made me notice it was when I cleaned them today. One held open foe easy cleaning. Put the romanian on my cleaning stand and the bolt wont hold. BW3, I will and see if that helps, thanks NOOB

Tn...Andy | 02-11-2007 09:23 PM
Re: ak47 question Ah.....then you want THIS link.....modify the safety lever. http://hunting.about.com/od/guns/ss/...ty_notch_2.htm

SAUM | 02-11-2007 10:10 PM
Re: ak47 question As always, top notch info from Andy.

grizzlyduck | 02-11-2007 10:32 PM
Re: ak47 question the piston and bolt carrier should have a little "wiggle" at the joint. some of the romy kits were pretty worn and the angle of the piston at the joint was too worn and the "wiggle" was excessive. all AKs when new will hold the bolt back under it's own tension and replacing the piston with a new one is kind of a pita. you have to find and pound out the hidden/welded over pin. then unscrew the piston and replace/drill new hold and re-pin, and then re-finish. not worth worrying about IMHO.

NOOB | 02-12-2007 07:32 AM
Re: ak47 question Thanks again everyone. NOOB

Libertarian_Guard | 02-12-2007 12:05 PM
Re: ak47 question Quote:
Originally Posted by NOOB (Post 506617) Thanks for the link TN, but I am talking about with the mag out. What made me notice it was when I cleaned them today. One held open foe easy cleaning. Put the romanian on my cleaning stand and the bolt wont hold. BW3, I will and see if that helps, thanks NOOB
Pull the bolt open. While holding the bolt fully open, slowly pull down on the trigger. While continuing to hold the trigger down, gradually release the bolt and slowly let it move forward. It will move forward a slight bit and stay locked open.

NOOB | 02-12-2007 05:34 PM
Re: ak47 question Quote:
Originally Posted by Libertarian_Guard (Post 507044) Pull the bolt open. While holding the bolt fully open, slowly pull down on the trigger. While continuing to hold the trigger down, gradually release the bolt and slowly let it move forward. It will move forward a slight bit and stay locked open.
That works wonderfully. Thanks NOOB

All times are GMT -4. The time now is 10:17 AM. |

Powered by vBulletin® Version 3.8.4
Copyright ©2000 - 2010, Jelsoft Enterprises Ltd.
Copyright = None use it and Link to GIM