Gold & Silver Forum (http://goldismoney.info/forums/index.php)
- Firearms (http://goldismoney.info/forums/forumdisplay.php?f=159)
- - How do I take apart my Remington 870?! (http://goldismoney.info/forums/showthread.php?t=358141)

erocktxmade | 03-13-2009 03:33 PM
How do I take apart my Remington 870?! OK I shot the Remington yesterday and it was beautiful. About 40 degrees out and my left hand kinda hurts from the recoil from the slide. Ran Remington and Winchester 00 Buck through and was mowing down plants and whatnot. ANYway I wanna take it apart and clean it. I tried before firing it and the magazine cap directly in front of the slide would not budge. After shootong I could move it a little. Now the next day it will not budge again. What do I unscrew? The cap directly infront of the slide? What about the piece that connects the barrel and magazine tube together with an X next to the screw? Do I do anything with that? What do I actually unscrew? Any help would be great! Thanks! Here is the gun in question: http://i55.photobucket.com/albums/g1...e/IMG_8114.jpg

Between The Wheels | 03-13-2009 03:51 PM
Re: How do I take apart my Remington 870?! http://www.alpharubicon.com/leo/870brian.htm http://www.learnaboutguns.com/2008/0...ng-video-clip/

erocktxmade | 03-13-2009 03:56 PM
Re: How do I take apart my Remington 870?! OK I have seen the videos and all that but the magazine cap screw will not budge! I even wrapped it in a towel and used pliers but will not move. It moved a little after shooting it but now it seems stuck!

End of Hope | 03-13-2009 05:44 PM
Re: How do I take apart my Remington 870?! You Tube
You Tube
You Tube
You Tube

bonaparte | 03-13-2009 08:12 PM
Re: How do I take apart my Remington 870?! Quote:
Originally Posted by erocktxmade (Post 1623819) OK I shot the Remington yesterday and it was beautiful.
That's great. I got mine yesterday too. Haven't shot it yet, but the video was helpful.

JJ_ | 03-13-2009 08:19 PM
Re: How do I take apart my Remington 870?! Hey dood- There's a screw that secures the clamp that holds the Mag tube to the barrel. you gotta get that clamp off first. then it comes off... l learnt that the hard way http://goldismoney.info/forums/pictu...&pictureid=220 :banghead: I'll try to get you a pic of it

erocktxmade | 03-13-2009 08:28 PM
Re: How do I take apart my Remington 870?! Son of a bitch....you are right. So much for Google. Thanks man! Comes off by hand after that! :565: Quote:
Originally Posted by JJ ShortStroke (Post 1624321) Hey dood- There's a screw that secures the clamp that holds the Mag tube to the barrel. you gotta get that clamp off first. then it comes off... l learnt that the hard way http://goldismoney.info/forums/pictu...&pictureid=220 :banghead: I'll try to get you a pic of it

Elvis | 03-13-2009 08:29 PM
Re: How do I take apart my Remington 870?! You may need to place the butt on the floor, grab on to the barrel and push it down a bit to take pressure off the end cap. Unloaded weapon, of course.

JJ_ | 03-13-2009 08:41 PM
Re: How do I take apart my Remington 870?! http://i284.photobucket.com/albums/l...e/100_4445.jpg Here's the screw: http://i284.photobucket.com/albums/l...e/100_4447.jpg

JJ_ | 03-13-2009 08:44 PM
Re: How do I take apart my Remington 870?! Quote:
Originally Posted by erocktxmade (Post 1624338) Son of a bitch....you are right. So much for Google. Thanks man! Comes off by hand after that! :565:
HA! Google aint sh..quat!:565: It's a real PITA till you figure that part out.

Usury | 03-14-2009 11:05 PM
Re: How do I take apart my Remington 870?! Cool....I picked up a Marine Magnum today.....it's reeeeeal nice.

loopy | 03-14-2009 11:14 PM
Re: How do I take apart my Remington 870?! Quote:
Originally Posted by erocktxmade (Post 1623819) OK I shot the Remington yesterday and it was beautiful. About 40 degrees out and my left hand kinda hurts from the recoil from the slide. Ran Remington and Winchester 00 Buck through and was mowing down plants and whatnot. ANYway I wanna take it apart and clean it. I tried before firing it and the magazine cap directly in front of the slide would not budge. After shootong I could move it a little. Now the next day it will not budge again. What do I unscrew? The cap directly infront of the slide? What about the piece that connects the barrel and magazine tube together with an X next to the screw? Do I do anything with that? What do I actually unscrew? Any help would be great! Thanks! Here is the gun in question:
See that Owner's Manual in your photo? Try cracking it open. Everything you need to know is in there :bear_tongue:

JJ_ | 03-14-2009 11:23 PM
Re: How do I take apart my Remington 870?! Quote:
Originally Posted by loopy (Post 1625964) See that Owner's Manual in your photo? Try cracking it open. Everything you need to know is in there :bear_tongue:
ACTUALLY - these are modified Mag Tubes... The owners manual does not include a breakdown for that componet. I've got the same manual.

loopy | 03-14-2009 11:37 PM
Re: How do I take apart my Remington 870?! Quote:
Originally Posted by JJ ShortStroke (Post 1625977) ACTUALLY - these are modified Mag Tubes... The owners manual does not include a breakdown for that componet. I've got the same manual.
Me too. Instructions for the extension kit came on an insert with the manual. looky looky :bear_tongue: http://home.comcast.net/~olimar/manual.jpg

JJ_ | 03-15-2009 01:25 AM
Re: How do I take apart my Remington 870?! I dont remember seeing it -- you're gonna make me go look now... arrgh.. its in the attic too -:banghead: Quote:
Originally Posted by loopy (Post 1626005) Me too. Instructions for the extension kit came on an insert with the manual. looky looky :bear_tongue: http://home.comcast.net/~olimar/manual.jpg

All times are GMT -4. The time now is 10:51 AM. |

Powered by vBulletin® Version 3.8.4
Copyright ©2000 - 2010, Jelsoft Enterprises Ltd.
Copyright = None use it and Link to GIM