Gold & Silver Forum (http://goldismoney.info/forums/index.php)
- Firearms (http://goldismoney.info/forums/forumdisplay.php?f=159)
- - K31 Swiss safety issue (http://goldismoney.info/forums/showthread.php?t=412250)

gypsybiker45 | 10-01-2009 09:06 PM
K31 Swiss safety issue I recently bought a K31 , question is, although this rifle appears to be in awesome shape, Im kind of afraid to fire it off! has any issues been found with these straight pull bolts flying into someones face? I now it sounds paranoid,the gun seems to cycle fine. and i see it locks when pushed forward.

desertjack | 10-01-2009 10:39 PM
Re: K31 Swiss safety issue I have two and they both shoot and function fine. You could always have a gunsmith kick the tires on it before you fire it if it will set your mind at ease. Once you do fire it you will like the straight pull bolt system.

Glass | 10-01-2009 10:41 PM
Re: K31 Swiss safety issue you got my interest up so I googled this review up: http://www.thefiringline.com/forums/...ad.php?t=94099 The second con suggests that slightly more force is required than normal to ensure the bolt has ridden home and fully locked. But then further down the thread people are suggesting not the gun but the ammo might cause this. Sounds like a fine gun to me with very good accuracy with the right ammo. Any chance of a pic?

Glass | 10-01-2009 10:56 PM
Re: K31 Swiss safety issue Now you got me interested. Wonder if I could get one of these here in the downunder You Tube
You Tube

____hoot____ | 10-02-2009 03:22 AM
Re: K31 Swiss safety issue Tie it to a tree and pull a cord from behind a bunker. I had one of these back in the 60-70s that was rechambered for 308[7.62 NATO]. Scary now that I think about it; but it never even hickupped pushing that .308 slug down a .300 bore barrel. My dad had bought it from a mail order outfit back in about 1960 for $29.95 with a dinky 4 power scope and passed it on to me. We got to wondering in later years if they had bothered to bore out that barrel to .308 when they rechambered it? I had shot a couple deer with it and I know that he had got a big 11 point withit in 61. Sold it sometime in the late 70s.

CrufflerJJ | 10-02-2009 10:39 AM
Re: K31 Swiss safety issue 1 Attachment(s) Quote:
Originally Posted by gypsybiker45 (Post 1950561) I recently bought a K31 , question is, although this rifle appears to be in awesome shape, Im kind of afraid to fire it off! has any issues been found with these straight pull bolts flying into someones face? I now it sounds paranoid,the gun seems to cycle fine. and i see it locks when pushed forward.
These are VERY safe. If the bolt serial number matches the receiver serial number, you're almost guaranteed safe headspace. Note that I would NOT say this about your usual Mauser or Mosin Nagant rifle. We're talking Swiss craftsmanship here, from the metal to the wood. The K31 is a great example of Swiss craftsmanship at its finest. The Swiss military also forced their troopies to maintain the rifles very well, and a soldier was forced to pay for a replacement barrel if he didn't maintain it properly! If the buttstock on your weapon looks "beat up" (with a scuzzier finish than the rest of the wood), see the attached picture to explain why. They also have GREAT trigger pulls, as issued. Not gritty at all. If you do any reloading with the 7.5x55 cartridge, you will need to watch your bullet seating depth. These rifles have a short throat, and seem to prefer "pointy" .308 projectiles. hoot - the bore diameter on K31 rifles is .308, not .300. Not sure about the older Swiss rifles.

TomD | 10-02-2009 11:03 AM
Re: K31 Swiss safety issue Quote:
Originally Posted by CrufflerJJ (Post 1951376) If you do any reloading with the 7.5x55 cartridge, you will need to watch your bullet seating depth. These rifles have a short throat, and seem to prefer "pointy" .308 projectiles.
Anyone who loads should understand ogive and have some way to measure distance to engage. I've always loved the 6.5x55, I assume it is related to the 7.5?

CrufflerJJ | 10-02-2009 01:17 PM
Re: K31 Swiss safety issue Quote:
Originally Posted by TomD (Post 1951424) Anyone who loads should understand ogive and have some way to measure distance to engage. I've always loved the 6.5x55, I assume it is related to the 7.5?
I don't know about the development history of the 6.5x55 vs 7.5x55, but (as you probably know), the 6.5x55 is Swedish (& Norwegian), while the 7.5x55 is Swiss. I've always been amazed at just how loooooong the bullet looks sticking out the end of a 6.5x55 case. As to reloaders understanding ogive, well....I suspect some know it better than others. When reloading for most common calibers, chamber throat/bullet ogive doesn't seem to be as critical as when reloading for the 7.5x55.

hypervel | 10-02-2009 04:48 PM
Re: K31 Swiss safety issue Shoot it. Really. Like asking if you shouldn't wear the Rolex 'cuz it might discolor your wrist. BTW, they're a little more slick (it seems to me) when they are loaded out. HAVE FUN, MAN! Go on, do it!

All times are GMT -4. The time now is 10:41 AM. |

Powered by vBulletin® Version 3.8.4
Copyright ©2000 - 2010, Jelsoft Enterprises Ltd.
Copyright = None use it and Link to GIM